The sensing distance of robot is <=7cm

The receiving part is attached at the back of the robot, the transporting part should be connected with power supply. Both of them are currently at IC.

